1. Flash the tsl-20.12.a-tep5-imx6-15.img sdcard image to an microSD card.

2. Insert the flashed micro sdcard into the tep5-imx6 target device
   Connect an hdmi cable from tep5-imx6 to your HDMI display panel
   Connect an internet-accessible ethernet cable to tep5-imx6

3. Hold S1 button while power on the device

4. Wait for about 30 seconds before release S1 button.

5. You should see TechNexion Software Loader on both HDMI and LVDS panel

